BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0141
Relative sending level

The command is used to state the relative transmission level (Lo) in the analogue interface to ELU-A.

##### Valid data

-12dBr to + 6dBr |  | (steps: 0,1 dBr) |
3 dBr (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005