BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0201
Allocate resources for programmable keys

This field allows you to select for how many programmable keys memory shall be reserved for selected extension. It is used to minimize allocated resources in the system for programming available extensions keys.

##### Valid data

Up to the last programmed key |  | If selected, only the memory blocks from the first up to the memory block required to store the data of the last programmed key in the list is reserved - 1 memory block consists of 15 keys - so if e.g. key A is programmed by BMS, the end user can program (if authorized) up to 15 keys (depending on the phone type) |
For all provided keys |  | If selected, then all the memory for this type of phone is reserved! The end user can program (if authorized) all the keys of his phone! |

The value of this command is not stored in the connected BusinessPhone system. The value is sent towards BusinessPhone after submitting this page in order to define the allowed key resources.

Default value is "for all provided keys".

Revision: J © Ericsson Enterprise 2005