BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1946
Forced message after timeout

This command states if a CONNECT or ALERTING message shall be sent to network 8 seconds after CALL PROCEEDING. This is to stop timer T303 and force the originating network to through connect the B-channel in order to give the caller the possibility to hear tones or announcements provided by the terminating party. The choice of CONNECT or ALERTING is network dependent.

##### Valid data

None |  |  |
Alert |  |  |
Connect |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005