BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3507
Reroute on no answer

This command defines the time after an incoming call to a PBX group, which is connected to an extension within the group, will be rerouted to the exit position. The time can be set between 1 and 255s. A value of 0 means that reroute on no answer is not activated.

In case that no exit position is defined (see command 3502), an external call will be rerouted to the exit position of the incoming trunk, an internal call will be released.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005