BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1315
MFE number plan for CLL

This command is used to set the number plan for Class of Call (CLL) code determination at MFE.

If no or a no existing number plan is programmed, the default number plan 0 (standard) is used.

#### Number Plan

Class of call | 0 | 1 | 2 | 3 | 4 | 5
Regional | 1-8 | 2-8 1xy,xy <>12 | 2-8 | 1-8 | 2-8 1xy,xy <>12 | 2-8
National | 9 | 9 | 9 | 9 | 9 | 9
International | 07 | 07 | 07 | 00 | 00 | 00
Special service | 0x,x<>7 | 0x,x<>7 112 | 0x,x<>7 1 | 0x,x<>0 | 0x,x<>0 112 | 0x,x<>0 1

Value = 00-15

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005