BusinessPhone Communication Platform 7.0
Dialogs

## DTMF Tones

This dialog allows you to define the number of tones, the frequency level, the level difference, the signal and the pause time for sending digits in DTMF mode.

To access the dialog, open the “System” menu in the Configuration directory tree. Now open the “Ring & tone signals” submenu and click on “DTMF Tones...”.

The following commands are available:

2610 |  | Number of DTMF tones

2611 |  | Level

2612 |  | Level difference

2613 |  | Signal time

2614 |  | Pause time

If you need more information about a setting or a field, click on the command link in brackets to open the online help system.

#### Actions

Submit |  | To send the settings to the system. |
Reload |  | To load the current system settings and to discard all entered data or changes. |

For more information, see also facility description Ring And Tone Signals (443/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005