BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x2F
Free Channel Check Failed

Default definition: |  | STOP |
Used by block: |  | OU |
Category: |  | MAINTENANCE |

This code is only used, when the periodic resource check, initiated by the supervision programs, failed. The warning indicates that the maximum number of free PCM channels, that has been available since the last check, is smaller than the anticipated number. The cause can be a program, that does not release resources correctly, or it can be that the system is used in a way, that locks up resources permanently. In the latter case, the warning code can be removed.

- D1:
- D2:
- D3: Undefined
- D4: Undefined

Revision: K © Ericsson Enterprise 2005