BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5204
Password for level 3

When system programming is executed from a system telephone, the user may log in at different authority levels. The lowest level contains only some selected commands while the highest level contains all commands of the system. The top level is the same level as the one used by BMS.

Using this command it is possible to determine the password for level 3. This level is the second highest authorization level.

The password may consist of maximum 5 digits (0-9).

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005