BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6305
Dialed number: suppress

Suppression of the last digits in the dialled number. The desired number of end digits can be stated with an “X” on the printout, if you for security reasons do not want to show the complete external number.

##### Valid data

00-15 |  |  |
00 |  | (default) all digits are registered |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005