BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1402
Time supervision of long register sign. alt. MFC/MFE outgoing

The command is used to determine the time for long supervision before the first digit and between the digits when dialing. Value 3-255 seconds.

Timeout results in disconnection/blocking, unless an open number has been received from the TCD-analysis, or a switch to speech state if an open number has been dialed.

Note

For decadic pulsing this time must not be less than the time required by the BTU-board to transmit the digit.

(See commands 1401 Number of digits with long dial supervision and 1403 Time supervision of short register sign. alt. MFC/MFE outgoing = the relationship between the number of digits and the time for supervision is adapted for possible standard number series for the line.)

For ISDN (BTUDP, BTUB) trunks the command is valid only in case of MLT-system configuration.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005