BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x27
Illegal PCM Channel Access

Default definition: |  | ERROR + TRIG |
Used by block: |  | OU |
Category: |  | DESIGNER |

OU denied the requested operation on the PCM channel. The cause may be an invalid channel number, an invalid channel state or an illegal job identity.

- D1: Channel number
- D2: Job identity (usually signal type ST) of the channel user
- D3: Undefined
- D4: Undefined

Revision: K © Ericsson Enterprise 2005