BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 53 ADFUNCTION

01h ADCLEAR |  | CP->RP Set max/min to current value |
02h ADSET_THRESHLD |  | CP->RP Set thresholds for warnings |
03h ADREAD_THRESHLD |  | CP->RP Read thresholds for warnings |
10h ADREAD_FAC_CUR |  | CP->RP Read current values |
11h ADREAD_FAC_MAX |  | CP->RP Read maximum values |
12h ADREAD_FAC_MIN |  | CP->RP Read minimum values |
13h ADREAD_SUP_CUR |  | CP->RP Read current values |
14h ADREAD_SUP_MAX |  | CP->RP Read maximum values |
15h ADREAD_SUP_MIN |  | CP->RP Read minimum values |
80h ADANSW_NAK |  | RP->CP Function not available |
81h ADANSW_ACK |  | RP->CP Requested function done |
82h ADLIM_FAC_CUR |  | RP->CP Out of limits message |
83h ADANSW_THRESHLD |  | RP->CP Answer upon ADREAD_THRESHLD |
90h ADANSW_FAC_CUR |  | RP->CP Answer with current values |
91h ADANSW_FAC_MAX |  | RP->CP Answer with maximum values |
92h ADANSW_FAC_MIN |  | RP->CP Answer with minimum values |
93h ADANSW_SUP_CUR |  | RP->CP Answer with current values |
94h ADANSW_SUP_MAX |  | RP->CP Answer with maximum values |
95h ADANSW_SUP_MIN |  | RP->CP Answer with minimum values |

Revision: F © Ericsson Enterprise 2005