BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0503
Notification number

The notification number is the corporate network or public number which willbe called by the outcall notification number facility.

The notification number consits of two part wich are discribed below.

#### First part must contains

- A valid trunk,
- a valid route,
- LCR or PNR internal directory number

#### Second part can be

- Any kind of number.

The only restriction of the notification number is, that the length of the two parts can not be longer than
24 digits.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005