BusinessPhone Communication Platform 7.0
Facilities

## Flexible CIL - Format

## Definition

The flexible CIL-format (valid from R13 onward) allows customers to create their personal call information logging records. All available CIL-data information are collected in a pool which may be selected to configure one´s own record.

## Use

There is a pool of CIL-data information which is needed by customers to create their own CIL-record matching to their external call accounting software. The customer can choose the information content and order in the CIL-record. The order of the call information logging record can be defined in the configuration table.

## Function

The customer has the opportunity to choose the CIL - data information field from a pool of available CIL - data information. There are specific commands which have to be set in the call information logging format table. These commands can only be programmed from BMS.

6420 |  | Flexible CIL- format

This command covers a configuration table, containing all available data fields and their numbers of characters. It is possible to scroll through the configuration table to have more information fields available.

From Release 13 onwards the following functions are enhanced in the CIL - data record:

Function | Description
TAG identifier | A TAG identifier is assigned to every external call. If more than one CIL record is generated, e.g. at Call Transfer, Conference, Call pick up, Partial Rerouting, Outcall notification etc., the associated CIL records can be identified by one TAG identifier. The TAG identifier consists of 2 bytes and is not forwarded via the private network. The TAG identifier is available within the CIL flexible format and is shown in a decimal notation (values from 1 to 65535).
Logging of CN (Corporate Network) transferred calls | If the connected CN party changes during conversation due to a CN transfer or termination of a CN conference, a CIL record for each connected party is generated in gateway nodes (CN / public network) or end-nodes within the CN.
Status information | Apart from the existing status information field a new field which is easy to expand, is introduced. The new information field comprises also the already existing status information, which makes the “old” information field unnecessary. The field is part of the flexible CIL format and is called “INFORMATION STATUS 3” and is shown in hexadecimal notation.
Call duration | If the timer runs more than 8 hours and 56 min, the exchange will send a TAG, to store the call duration of the CIL record temporarily.
Call originator / terminator information field | A new information field with call originator / terminator information is introduced. The field is part of the flexible CIL - format and is called “ORG/TERM DEFINITION”. It is shown in a hexadecimal notation.
End time / Call duration | The new information filed “END TIME - hh:mm:ss” and “CALL DURATION - hh:mm:ss” within the “CIL - flexible format” for “Call Duration” and “End Time” with the format HH:MM:SS is introduced. Hours, minutes and seconds are represented by two digits each.
DDI number translation | The translated numbers (up to 8 digits) are shown within the “CIL - flexible format” with the new fields “CALLERS NUMBER DDI” and “AUTHORISATION CODE DDI”. Beside the new fields, the “DIALED NUMBER CIL4” field is to be programmed in the “CIL - flexible format”.

## Capacity/Limitations

A call information logging record may contain a maximum of 30 data fields, whereby the total character lenght must not exeed 230 characters.

Note

Up to Release 12 only the CIL3HOTEL format could be sent via the CTI-link (Call CTI (out)). With command 6407 all bi-directional formats that are programmed by command 6403 can be sent via the CTI-link on channel 0.

## Programming

6403 |  | Format table

Note

The relevant values for the flexible CIL-format are Flexible CIL-Format (unidirectional) or
Flexible CIL-Format (bidirectional).

6420 |  | Flexible CIL- format

Note

The flexible CIL - Format allows a customer to create his personal call information logging record.

The format table will be expanded with the flexible CIL - format for uni- and bi- directional V.24 interface. For every format, special CIL - data are assigned, which may be selected and controlled by means of the call information logging record.

6407 |  | CIL-data via CTI-link

The following table shows the additional information fields which are implemented in the Flexible CIL:

No. | Additional Information fields | Value | Character
1 | Authorisation code CIL4 | 0-9999 | (4)
2 | B-number | 20 digits | (20)
3 | C-number | 20 digits | (20)
4 | Call date (mmdd) HIS | month-day (mmdd) | (4)
5 | Call duration | hour-min-min/10 (hmmm/10) | (4)
6 | Call duration | hour-min-sec (hhmmss) | (8)
7 | Call duration (minutes) HIS | 0000-9999 min (max. 0600) | (4)
8 | Call via facility CIL4 | 1 character | (1)
9 | Called number ASB | 1-20 digits | (20)
10 | Called number HIS | 14 digits | (14)
11 | Caller´s number CIL4 | 0-9999 | (4)
12 | Caller´s number HIS | 0-9999 | (5)
13 | Dialled number CIL2 | 20 digits | (20)
14 | End time HIS | hour min (hhmm) | (5)
15 | End time CIL4 | hour min (hhmm) | (4)
16 | HOTEL ALPHA EBC | EBC | (3)
17 | HOTEL ALPHA HIS | HIS | (3)
18 | Information status I CIL4 | 1 character | (1)
19 | Information status II CIL4 | 1 character | (1)
20 | Information status ASB | 1 character | (1)
21 | Meter pulses HIS | 0-9999 | (7)
22 | Sequence number+A HIS | 001A -999A | (4)
23 | Space 1 | Space,”SP” | (1)
24 | Space 5 | 5 space,”SP” | (5)
25 | Space 10 | 10 space,”SP” | (10)
26 | Transfer condition CIL4 | 2 digits | (2)

Revision: H © Ericsson Enterprise 2005