BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks

## Signal Types

Signal-type (ST) is a one byte code used by the central operating system to identify a “signal input” in a 6809 CP-program (JOB). Used in similar way in some RPs too.

##### Valid signal-types in ASB 150 02

- CP = 40h - FBh
- RP = 00h - 3Fh

Signal Type |  | Signal Type (hex) |  | Short Name |  | Comment |
82 |  | 52 |  | ARPRG |  | AR- Auto Redial prog. input |
83 |  | 53 |  | ARINP |  | AR- Auto Redial main input |
84 |  | 54 |  | ACPRG |  | AC - Account code, programming |
85 |  | 55 |  | MGOCN |  | MG - Outcall Notification |
86 |  | 56 |  | IPPRG |  | IP - Programming input |
87 |  | 57 |  | MGREC |  | MG - Conversation Recording |
88 |  | 58 |  | CBPRG |  | CB – Call Back, programming |
89 |  | 59 |  | ROPNR0 |  | RO – Private Network Router 0 |
90 |  | 5A |  | ROPNR1 |  | RO – Private Network Router 1 |
91 |  | 5B |  | ROPNR2 |  | RO – Private Network Router 2 |
92 |  | 5C |  | ROPNR3 |  | RO – Private Network Router 3 |
93 |  | 5D |  | ROOWN |  | RO – Own Location |
94 |  | 5E |  | CIBEG |  | CI - Caller List Prog. input |
95 |  | 5F |  | CIINP |  | CI - Caller List main input |
96 |  | 60 |  | OSTST |  | OS – Interface for test tool WILMER |
97 |  | 61 |  | OULQU |  | OU – The Load regulation Queue |
98 |  | 62 |  | AAINP |  | AA – Automated Attendant, main input |
99 |  | 63 |  | AABEG |  | AA – Automated Attendant, initialisation and programming |
100 |  | 64 |  | DEBEG |  | DI – Begin, initialisation |
101 |  | 65 |  | DEINP |  | DI – Normal input |
102 |  | 66 |  | DEPRG |  | DI – Programming |
103 |  | 67 |  | DEE2H |  | DI – E2-data interface |
104 |  | 68 |  | CTBEG |  | CT – Startup, Programming |
105 |  | 69 |  | CTINP |  | CT – Main input |
106 |  | 6A |  | EXBYP |  | EX – Bypassing Call Diversion |
107 |  | 6B |  | EXLOG |  | EX – Logon/off of Slave |
108 |  | 6C |  | EXVPN |  | EX – Virtual private networking |
109 |  | 6D |  | EXSHD |  | EX – Shutdown input |
110 |  | 6E |  | SUPRG |  | SU – Programming |
111 |  | 6F |  | OSOUPRG |  | OS & OU – Programming |
112 |  | 70 |  | CMBEG |  | CM – Call metering, programming and initialisation |
113 |  | 71 |  | EXMLT |  | EX – Multi Line Terminal |
114 |  | 72 |  | CABEG |  | CA – Cost, programming and initialisation |
115 |  | 73 |  | CAINP |  | CA – Cost Analysis, main input |
116 |  | 74 |  | CAPRG |  | CA – Cost, programming input |
117 |  | 75 |  | TNINP |  | TN – Test number, main input |
118 |  | 76 |  | EXLNR |  | EX – Last number redial, main input |
119 |  | 77 |  | EXTOG |  | EX – Toggle function, main input |
120 |  | 78 |  | MCINP |  | MC – Traffic input |
121 |  | 79 |  | LRBEG |  | LR – Initialisation |
122 |  | 7A |  | LRINP |  | LR – Traffic input |
123 |  | 7B |  | LRPRE |  | LR – Prefix |
124 |  | 7C |  | NABEG |  | NA – Programming and initialisation |
125 |  | 7D |  | NAINP |  | NA – Number Analysis |
126 |  | 7E |  | EXCOB |  | EX – Common Bell Extension |
127 |  | 7F |  | E2PRG |  | E2 - Programming input |
128 |  | 80 |  | OSRTC |  | OS – Real time clock handler |
129 |  | 81 |  | OSSPO |  | OS – OSHWI, Send to RP (SP-out) (must be 8100h; this value is defined in the test card (TSTX) |
130 |  | 82 |  | SXTRM |  | SX – Switch, transmission |
131 |  | 83 |  | SXMPU |  | SX – Switch, Multi party |
132 |  | 84 |  | E2BEG |  | E2 – Begin, initialisation |
133 |  | 85 |  | E2INP |  | E2 – Normal input |
134 |  | 86 |  | CEBEG |  | CE – Convert E2data, R1->R2, R2->R3, ... |
135 |  | 87 |  | SUINP |  | SU – Input for all signals |
136 |  | 88 |  | SDINP |  | SD – Distribution of SEIZ-messages |
137 |  | 89 |  | SDDIR |  | SD – Distribution on directory number |
138 |  | 8A |  | SDIND |  | SD – Input for message from RPs |
139 |  | 8B |  | ALPRG |  | AL – Alarm, programming |
140 |  | 8C |  | ADTRA |  | AD – Abbrev. dial traffic-input |
141 |  | 8D |  | CDSTA |  | CD – ACD statistics |
142 |  | 8E |  | PABEG |  | PA – Begin, initialisation |
143 |  | 8F |  | PAPRG |  | PA – Programming |
144 |  | 90 |  | CMINP |  | CM – standard input |
145 |  | 91 |  | EUINP |  | EU – Standard input |
146 |  | 92 |  | EUPRG |  | EU – Programming |
147 |  | 93 |  | TSBEG |  | TS – Begin, initialisation |
148 |  | 94 |  | TSINP |  | TS – Standard input |
149 |  | 95 |  | TRSER |  | TR – Service input |
150 |  | 96 |  | OMPRG |  | OM – Programming |
151 |  | 97 |  | OMWRN |  | OM – Warning ram-buffer examine |
152 |  | 98 |  | OMBEG |  | OM – Begin, initialisation |
153 |  | 99 |  | OMINP |  | OM – RP-communication, etc. |
154 |  | 9A |  | OMCOM |  | OM – Communication with PR |
155 |  | 9B |  | OMEPC |  | OM – Communication with PC and EPC |
156 |  | 9C |  | OMTST |  | OM – Test of instrument |
157 |  | 9D |  | ALINP |  | AL – Readout of alarm |
158 |  | 9E |  | ALALR |  | AL – Receive alarm |
159 |  | 9F |  | OMOWN |  | OM – Internal signalling |
160 |  | A0 |  | EXBEG |  | EX – Begin, initialisation |
161 |  | A1 |  | EXINP |  | EX – Traffic input |
162 |  | A2 |  | EXKTR |  | EX – Key translator |
163 |  | A3 |  | EXPRG |  | EX – Programming |
164 |  | A4 |  | EXCHG |  | EX – Traffic input for programming |
165 |  | A5 |  | EXDSP |  | EX – Display information |
166 |  | A6 |  | EXAUT |  | EX – Authority codes |
167 |  | A7 |  | EXMAI |  | EX – External voice mail |
168 |  | A8 |  | PRBEG |  | PR – Begin, initialisation |
169 |  | A9 |  | PRINP |  | PR – Traffic input |
170 |  | AA |  | PRKDH |  | PR – Keyboard and display handler |
171 |  | AB |  | PRSPP |  | PR – Support |
172 |  | AC |  | PRCMD |  | PR – Command |
173 |  | AD |  | PRIND |  | PR – Individual programming |
174 |  | AE |  | TRINP |  | TR – Traffic input |
175 |  | AF |  | TRPRG |  | TR – Programming |
176 |  | B0 |  | CBBEG |  | CB – Begin, initialisation |
177 |  | B1 |  | CBINP |  | CB – Traffic input |
178 |  | B2 |  | TDBEG |  | TD – Begin, initialisation |
179 |  | B3 |  | TDPRG |  | TD – Programming |
180 |  | B4 |  | ROBEG |  | RO – Begin, initialisation |
181 |  | B5 |  | ROINP |  | RO – Traffic input |
182 |  | B6 |  | ROPRG |  | RO – Programming |
183 |  | B7 |  | GHBEG |  | GH – Begin, initialisation |
184 |  | B8 |  | GHINP |  | GH – Traffic input |
185 |  | B9 |  | GHPRG |  | GH – Programming |
186 |  | BA |  | ADBEG |  | AD – Begin, initialisation |
187 |  | BB |  | ADINP |  | AD – Traffic input |
188 |  | BC |  | ADPRG |  | AD – Programming |
189 |  | BD |  | MUBEG |  | MU – Begin, initialisation |
190 |  | BE |  | MUINP |  | MU – Traffic input |
191 |  | BF |  | MUPRG |  | MU – Programming |
192 |  | C0 |  | GPBEG |  | GP – Begin, initialisation |
193 |  | C1 |  | GPINP |  | GP – Traffic input |
194 |  | C2 |  | GPPRG |  | GP – Programming |
195 |  | C3 |  | CDBEG |  | CD – ACD Begin, initialisation |
196 |  | C4 |  | CDINP |  | CD – ACD Traffic input |
197 |  | C5 |  | CDPRG |  | CD – ACD Programming |
198 |  | C6 |  | TJOB0 |  | TJ- Test job, handles CPJOB from TSTX |
199 |  | C7 |  | TJOB1 |  | TJ – Test job, factory testing and others |
200 |  | C8 |  | TJOB2 |  | TJ – Test job, factory testing and others |
201 |  | C9 |  | VPBEG |  | VP – Begin, initialisation |
202 |  | CA |  | VPINP |  | VP – Traffic input |
203 |  | CB |  | VPPRG |  | VP – Programming |
204 |  | CC |  | DIBEG |  | DI – Begin, initialisation |
205 |  | CD |  | DIINP |  | DI – Normal input |
206 |  | CE |  | DIPRG |  | DI – Programming |
207 |  | CF |  | DIE2H |  | DI – E2-data interface |
208 |  | D0 |  | EXEXT |  | EX - Individual external diversion |
209 |  | D1 |  | RSINP |  | RS - Register signal |
210 |  | D2 |  | CLPRG |  | CL – Programming |
211 |  | D3 |  | COBEG |  | CO – Begin, initialisation |
212 |  | D4 |  | COINP |  | CO – Traffic input |
213 |  | D5 |  | COPRG |  | CO – Programming |
214 |  | D6 |  | BIBEG |  | BI – Begin, initialisation |
215 |  | D7 |  | BIINP |  | BI – Traffic input |
216 |  | D8 |  | BIPRG |  | BI – Programming |
217 |  | D9 |  | OPBEG |  | OP – Begin, initialisation |
218 |  | DA |  | OPINP |  | OP – Traffic input |
219 |  | DB |  | OPPRG |  | OP – Programming |
220 |  | DC |  | OPQUE |  | OP – Queue, traffic input |
221 |  | DD |  | CLIOP |  | CL – I/O-port handler |
222 |  | DE |  | FNINP |  | FN – Traffic input |
223 |  | DF |  | FNPRG |  | FN – Programming |
224 |  | E0 |  | MGBEG |  | MG – Begin, initialisation |
225 |  | E1 |  | MGINP |  | MG – Traffic input |
226 |  | E2 |  | MGPRG |  | MG – Programming |
227 |  | E3 |  | INBEG |  | IN – Begin, initialisation |
228 |  | E4 |  | ININP |  | IN – Traffic input |
229 |  | E5 |  | INPRG |  | IN – Programming |
230 |  | E6 |  | ANBEG |  | AN – Begin, initialisation |
231 |  | E7 |  | ANINP |  | AN – Traffic input |
232 |  | E8 |  | ANPRG |  | AN – Programming |
233 |  | E9 |  | VMBEG |  | VM – Begin, initialisation |
234 |  | EA |  | VMINP |  | VM – Traffic input |
235 |  | EB |  | VMPRG |  | VM – Programming |
236 |  | EC |  | VMERA |  | VM – Erase |
237 |  | ED |  | VMSUP |  | VM – Supervision |
238 |  | EE |  | CLINP |  | CL – Input |
239 |  | EF |  | ACINP |  | AC – Traffic input |
240 |  | F0 |  | HOBEG |  | HO – Begin, initialisation |
241 |  | F1 |  | HOINP |  | HO – Traffic input |
242 |  | F2 |  | HOPRG |  | HO – Programming |
243 |  | F3 |  | PGBEG |  | PG – Begin, initialisation |
244 |  | F4 |  | PGINP |  | PG – Traffic input |
245 |  | F5 |  | PGPRG |  | PG – Programming |
246 |  | F6 |  | REBEG |  | RE – Begin, initialisation |
247 |  | F7 |  | REINP |  | RE – Traffic input |
248 |  | F8 |  | REPRG |  | RE – Programming |
249 |  | F9 |  | BISIL |  | BI – Silent intrusion |
250 |  | FA |  | LSINP |  | LS – Link supervision |
251 |  | FB |  | EDINP |  | ED – Text editing for extensions |
254 |  | FE |  | INIT |  | Value used as identifier for any at 'init' |
255 |  | FF |  | EXIT |  | Value used as identifier for OS at job-exit |

Revision: F © Ericsson Enterprise 2005