BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1301
Incoming digit transmission

The command states how the digits are sent by the working exchange.

The initial value depends on the type of the BTU.

The following initial values are available:

Type of BTU: |  | Value: |
BTU-A |  | 0 |
BTU-C |  | 0 |
BTU-E |  | 0 |
BTU-D |  | 2 |

0 = Decadic impulsing |  |

1 = DTMF |  |

2 = MFC |  |

3 = No sending of digits |  |

4 = MFE1 (2/5) |  |

5 = MFE2 (2/6) |  |

Value = 0-5

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005