BusinessPhone Communication Platform 7.0
Dialogs

## Port configuration data

Note

This feature is only available for BusinessPhone V5.0 (ASB 150 02 R12) or later versions!

In this table, you can view and edit up to 15 entries for the port configuration.

To access the Port Configuration Data dialog, open the “System” menu in the Configuration directory tree. Then open the “System parameters” submenu and click on “IPU Board Data...”. The Basic IPU Data dialog appears. On top of the dialog, you find a navigation bar. Click on “Ports” to open the dialog.

The following commands are available:

2161 |  | Application

2162 |  | Port number

If you need more information about a field, click on the command link in brackets on top of the table to open the online help system. See also System Description (1551-ASB 150 02 Uen).

### Other IPU Board Data dialogs

On top of the dialog, you find a navigation bar that provides access to the following IPU Board Data dialogs:

- Basic Data

- To open the Basic IPU Data dialog.

- Ports

- The dialog you view right now.

- Gatekeeper

- To open the Gatekeeper Data dialog.

- H.323 extension gateway

- To go to the H.323 Extension Gateway Data dialog.

- Licensing

- To go to the Voice Channel Licensing dialog.

- Board Configuration

- To open the Board Configuration dialog.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

Revision: B © Ericsson Enterprise 2005