BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2161
Application

Specifies the feature and/or protocol, associated with the TCP port.(command 2162)

##### Valid data

0 |  | No application (i.e. the port is not used) |
1 |  | I/O port 1 (e.g. for VCom, etc.) |
2 |  | I/O port 2 (e.g. for VCom, etc.) |
3 |  | I/O port 3 (e.g. for VCom, etc.) |
4 |  | I/O port 4 (e.g. for VCom, etc.) |
5-100 |  | Spare |
101 |  | ASB 150 02 IP gateway |
102-255 |  | reserved |

Note

The table is already predefined with the available applications in ASB 150 02, so there is no need to modify the table so far.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005