BusinessPhone Communication Platform 7.0
Installation Instruction ASB 150 02

## Boards for ASB 150 02

This document describes all the ASB 150 02 boards from Release R3 upwards, which still might be installed at the customer site. Some of these boards are already phased out and can not be ordered anymore.

### Handling of PBAs

Service personnel shall always connect themselves to a protective ground terminal point to prevent damage caused by static discharges.

Note

Boards with Electrostatic Sensitive Devices (ESD) are marked with a sign.In the interest of quality and reliability of the system boards, always handle static sensitive boards with special care. Always use a wrist strap connected to a low resistance ground e.g. provided on the cabinet:
Use portable equipment LYA 30101 as a protection against electrostatic discharges. For safety reasons the wrist strap should be equipped with a 1 MOhm serial resistor.

Some of the benefits of ESD protection are:

- less failures/service calls
- lower maintenance costs
- higher customer satisfaction

### Connection fields on the PBAs

### Board position numbering

#### BP 250 (Cabinet: BDV 113 08)

Board position numbering for:

- Cabinet 0: position 0,1 --- 8.
- Cabinet 1: position 16,17 --- 24.
- Cabinet 3: position 48,49 --- 56.

#### BP 128i (Cabinet: BDVBS 101 06)

Board position numbering for:

- Cabinet 0: position 0,1,2,3,4.
- Cabinet 1: position 16,17,18,19,20.

#### BP 50 and BP Compact (Cabinet: BDVBS 101 05)

Board position numbering for:

- Basic unit: position 0,1,2,3,4.

### Placing of boards

The cabinets BDV 113 08, BDVBS 101 05 and BDVBS 101 06 are prepared for arbitrary furnishing of boards belonging to the ASB 150 02 system but certain constraints should be considered for best performance results.

#### BDV 113 08

The cabinet 0 and the two optional cabinets 1 and 2 have to be equipped as follows:

Pos. 0 |  | Reserved for CPU-D_

Pos. 1-8, 16-24, 48-56 |  | Available for arbitrary PBA configuration like ELU-_,MFU, VMU-D, VMU-HD, AUX_, BTU-_ , REG, IC-CU_ and IC-LU. The latter one requires PUB 5 or higher.

When installing boards with ground brackets in a cabinet of an earlier release of BDV 113 08, which was not prepared for them, take out the screws of the ground brackets at the top and bottom of the boards. Then bend the bracket at the top slightly away from the cabinet to allow a clearance for the front cover to slip on correctly.

#### BDVBS 101 06

The cabinet 0 and the optional cabinet 1 have to be equipped as follows:

Pos. 0 |  | Reserved for CPU-D_

Pos. 1-4 ,16-20 Available for arbitrary PBA configuration like ELU-_,MFU, VMU-D, VMU-HD, AUX_, BTU-_ , REG, IC-CU_, IC-LU, IPU and IAS. |  |

Note

The cabinet BDVBS 101 06 does not support ELU-C boards

#### BDVBS 101 05

##### BusinessPhone 50

This single cabinet has to be equipped as follows.

Pos. 0 |  | Reserved for CPU-D_

Pos. 1-4 |  | Available for arbitrary PBA configuration like ELU-_,MFU, VMU-D, VMU-HD, AUX_, BTU-_ , REG, IC-CU_, IC-LU (requires PUB 50 R4A or higher) IPU and IAS.

##### BusinessPhone Compact

This single cabinet solution supports five board positions however the CPU-D5C supports only the board positions 1 and 2 or all board types, position 3 and 4 can only be used for the integrated cordless boards (IC‑LU).

In conjunction with an additional software license the CPU-D5C can be upgraded to support all board positions.

Pos. 0 |  | Reserved for CPU-D5C

Pos. 1-2 |  | Available for arbitrary PBA configuration like ELU-_,MFU, VMU-HD, AUX_, BTU-_ , REG, IC-CU_, IC-LU, IPU and IAS.

Pos. 3-4 |  | IC-LU

Note

The cabinet BDVBS 101 05 does not support ELU-C boards

#### Board specific positioning

All boards except the CPU-D_ can be exchanged under power provided that the board is replaced by a board of the same type and configuration. New boards e.g. to upgrade the system, can be installed under power in a free slot of the cabinet.

##### IPU boards

If an IPU is equipped with one DSM2 or two DSM1, then the very last position of a cabinet has to be used. If any other position has to be chosen or in case of multiple IPUs then the next right hand board position of the IPU must be left free. This limitation does not apply for the BP 128i (Cabinet: BDVBS 101 06)

ASB 150 02 R12 supports one IPU with maximum 8 voice channels only.

##### IC-CU_ and IC-LU boards

The Integrated Cordless system has to be installed within one cabinet. BMS cannot detect IC-LU boards installed in the system so it is advisable to insert these boards to the right of the IC-CU_ board. IC-LU boards can be removed and replaced without needing to shut down the exchange.

##### IAS

For the IAS the very last possible position of a cabinet (pos 7 or 23 or 55 in case of a BP 250 cabinet, pos 3 in case of a BP 50 cabinet) has to be used. If any other position has to be chosen then the next right hand board position of the IAS must be left free. This limitation does not apply for BP 128i (Cabinet: BDVBS 101 06).

##### Sub-equipped boards

Install sub-equipped boards in the last position after the standard boards to enable easy upgrading without having to re-number trunks and extensions.

#### EMC

The ferrites, with the ERICSSON ordering number STF 82 601, should be situated close to the slot where the cables are led out of the cabinet. Two turns through the ferrite core are sufficient to comply with EN 55022 Class B and to avoid disturbances in non-industrial, residential (home) usage.

#### More Information

CPU‑D2 (ROF 157 5118/2) CPU‑D3 (ROF 157 5118/3) AUX2 (ROF 1575 119/2) AUX3 (ROF 1575 119/3)

CPU-D4 (ROF 157 5124/1)

CPU-D5 (ROF 157 5124/2)
CPU-D5C (ROF 157 5124/3)

BTU-A (ROF 157 5110/_)

BTU-A2 (ROF 157 5120/_)

BTU-C (ROF 157 5111/_)

Connection of CM-boards on BTU-A and BTU-C

Power failure circuit (PFC) on BTU‑A/BTU‑A2 and BTU-C

BTU-B (ROF 157 5121/_)

BTU-B2 (ROF 157 5121/_)

BTU-D (ROF 157 5112/1) & REG (ROF 157 5112/2)

BTU-E (ROF 157 5113/_)

ELU-C (ROF 157 5115/1)

ELU-A (ROF 157 5114/_)

ELU-D3 (ROF 157 5130/_)

MFU (ROF 157 5132/_)

VMU-HD (ROF 157 5126/_)

VMU-D (ROF 157 5117/1)

IPU (ROF 157 5133/1)

IAS (ROF 157 5134/1)

Revision: J © Ericsson Enterprise 2005