BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2340
Traffic check at conference

This command states how the traffic group check should be executed for normal conference calls.

Alternatives:

0 = It is only necessary that the conference leader is open to call or receive calls from all parties in the conference. |  |

1 = The conference leader has to be open to call or receive calls from all parties, and there must be at least one direction open between all other parties in the conference. |  |

2 = The traffic group has to be open in both directions between all parties in the conference. |  |

3-9 Reserved. |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005