BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1317
Complete called party number length

This command states the total amount of digits in called party number which is required before a call setup/seizure is started to the network. The digit dialling is supervised with register timer in accordance to command 1403 Time supervision of short register sign. alt. MFC/MFE outgoing. If the timer elapses then the call-setup is started without any further number length control.

Value = 1-32

not programmed = blank (ordinary called number handling)

In case of CN calls the C-NL category for private network router (commands 9115 Complete called party NL 1, 9125 Complete called party NL 2, 9140 4-th route choice, 9145 Complete called party NL 4) overrides this trunk category.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005