BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0118
Guest extension?

In hotels, the extensions are divided into guest extensions and service extensions.

This command states whether the extension shall be a guest extension (Y) or a service extension (N).

As a rule guest extensions are assigned as special telephones. They have access to facilities such as wake-up and do not disturb, but not to facilities such as follow-me and information.

For hotel commands see command group 80.

It is not possible for a digital guest extension to program the second key-level. So the user can not use it. At also, an extension can not be an guest extension and a data extension at the same time.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005