BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0155
Disable call state message to line?

This command enables call state information to the line, i.e when a PC is connected to TAU as a PES equipment then this command has to be set to NO.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005