BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5623
LCR directory number

This command will be used to define the internal directory number to request an LCR-analysis.

This directory number should be dialled as a prefix before the external number to indicate that an LCR-analysis should be done. In this case it does not matter whether or not the trunk is programmed to require LCR-analysis or whether the originator has set the override control.

See:

Command 0148 Automatic display of metering info? |  | Override LCR control |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005