BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6701
I/O Port

This command can be used to define the board number and the individual number of the I/O port, where call metering data should be output.

Value:

ppiii |  |

pp: Board position |  |

iii: Individual number of a V24 (IO unit) port |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005