BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4311
Keep answered text

This command states how many answered text messages can be saved. Thus, the size of the part of the E2 memory to be used for answered messages can be determined here. This, of course, reduces the space for unanswered messages correspondingly.

Value 0 means that an unanswered message will be erased automatically upon answer except in case of a display telephone, where the message is erased by means of a command. Value 1-99 specify the number of answered messages saved. They can be accessed by means of a special procedure.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005