BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0xA9
SC-Message Buffer Overwrite

Default definition: |  | ERROR |
Used by block: |  | SP |
Category: |  | DESIGNER |

The serial communication processor (SP) has not received a CSMERY for the next D$SCMx field to use, but all D$SCMx fields are not busy. This indicates, that CP has executed the D$SCMx fields in incorrect order or made some other error. In order not to ‘loose’ this D$SCMx field, SP overwrites it with a new message from RP.

- D1:
- D2: D$SCMx field number
- D3: Undefined
- D4: Undefined

Revision: K © Ericsson Enterprise 2005