BusinessPhone Communication Platform 7.0
Facilities

## Diversion when charging the cordless phone

## Definition

The DT590 cordless phone has the possibility to divert incoming calls to a pre programmed divertee (answering) position when it is placed in the charger.

The used divertee position is the common one which is used for the feature Diversion direct, Diversion On Busy, Diversion On No Reply as well as Call deflection

## Use

When the cordless phone is placed in the charger, it will usually not be used, as the user is either not available (e.g. out of the working hours) or the battery is empty. During this period the cordless phone the user will normally diverte the phone to an alternative divertee position by using the Diversion direct or Individual internal/external diversion. When activating the DT590 specific feature “Redirect in charger”, incoming calls will automatically be diverted when the cordless phone is placed in the charger. No further diversion feature needs to be activated.

The feature “Redirect in charger” is a cordless phone specific feature which means that the ASB 150 02 system has no information whether or not this feature is activated. The diversion takes place on call base which means when the feature is activated on the cordless phone and it is placed in the charger, all incoming calls will be released by the cordless phone immediately. This immediate release during the call setup forces the ASB 150 02 to divert the call to the pre programmed divertee position.

### Diversion rules

1. If command 0112 Destination for fixed diversion is not set, external incoming calls will be rerouted to the trunk reroute position, internal calls will be released.
2. If the DT590 phone is a logged on Slave in a Tandem configuration incoming calls will only be presented at the Master. To make sure that a further diversion can take place on the Master (e.g. on no reply) the command 0123 Repeated call diversion? has to be set on the Master.
3. If the DT590 phone is a logged on Slave in a Tandem configuration and the Master is a logged off IP-client, incoming calls will be diverted according to the command 0112 Destination for fixed diversion.
4. If the DT590 phone is a not logged on Slave in a Tandem configuration, incoming calls to the Slave (due to the command 0165 Diversion on no reply to slave ) will be diverted according to the command 0112 Destination for fixed diversion.

## Operation

### Activate

1. Press the MENU key
2. Select the “Toolbox” tab
3. Select the menu item “In charger mode” and press the YES key

- The following options are available:

- Redirect
- Off

1. Select “Redirect” and press the YES key

### Deactivate

Use the same procedure as for activating the feature with the difference that in step 4 the option “Off” has to be selected instead of “Redirect”.

## Capacity

Each extension in the system can be assigned a divertee position.

The divertee position is common for all types of diversion, direct, busy, no reply, call deflection and when charging the cordless phone.

## Limitations

The status of the feature (activated) is not indicated in the idle display.

## Programming

0112 |  | Destination of fixed diversion

0123 |  | Repeated call diversion?

## Equipment

### Telephone type:

DT590

### Central Software:

Release R14 R4A or higher

Note

In CSW versions below R14 R4A the feature must not be activated on the cordless phone, as all incoming calls will automatically be released when the cordless is placed in the charger.

Revision: A © Ericsson Enterprise 2005