BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0185
Individual external diversion at external calls

This command defines whether or not an individual external diversion as well as a follow me to an external common abbreviated number shall be performed at incoming external calls.

If the extension is a master and a member of a tandem configuration, the command data shall be copied to the slave and blocked for the slave's further use.

Note

To enable the user to use the individual external diversion, the command 3093 Individual external diversion

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005