BusinessPhone Communication Platform 7.0
Facilities

## Hotel General

## Definition

ASB 150 02 can be utilised as a communication system for hotels.

## Use

Extensions can be freely distributed among:

- administration extensions
- service extensions
- guest-room extensions

## Operation

Check-in/-out is possible from:

- an DBC 223, DBC 213 or DBC 662 telephone (see Reception Extension)
- Hotel computer (see Hotel Computer)

Guests may utilise the following facilities:

- Do not disturb
- Diversion on busy
- Diversion on no reply
- Wake-up
- Message system
- Mailbox system
- Direct call keys to various service functions
- Group listening
- Background music

Service telephones can be grouped with the possibility of diversion to other service telephones.

### Hotel Computer

A hotel computer can be used to render various administrative functions in a hotel more effective.

ASB 150 02 is also adapted for the exchange of information with other (different) hotel computers.

This means that the hotel computer must be configured, whereby information exchange and protocol agree with one of the protocols offered by ASB 150 02.

## Capacity

ASB 150 02 can have a maximum of 288 extensions in a hotel configuration.

Revision: J © Ericsson Enterprise 2005