BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1916
Overlap receiving of called party number

The command is used to define the digit receiving method for current ISDN-link. It states whether all incoming digits are within the call setup message from the network or whether the digits are received within separate messages from the network.

The following digit receiving methods are available in BTUB and BTUDP:

- NO: No overlap digit receiving. Overlap digit receiving procedure not used, all digits are within call setup message (en-block procedure).
- YES: Overlap digit receiving. Overlap digit receiving procedure is used, digits are received within separate messages from the network.

Country specific settings

Country | Value
Australia | NO
Austria | YES
Belgium | YES
Italy | YES
Netherlands | YES
Sweden | ---
Spain | ---
Finland | YES
Denmark | YES
New Zealand | NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005