BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1404
Wait time before start to send digits when no PTS

The command is used to determine the shortest time required by the parent exchange to receive digits for outgoing calls from ASB 150.

The function is used when the parent exchange does not send any proceed- to-send signal as acknowledgement.

Value 0-255 seconds. 0 = instant result.

(Command 1307 PTS-signal from parent exchange? states whether there will be a proceed-to-send signal from the exchange.)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005