BusinessPhone Communication Platform 7.0
Installation Instruction ASB 150 02 > Boards for ASB 150 02

## VMU-HD (ROF 157 5126/_)

To install unpack the VMU-HD board with the mounted Compact Flash Card. The Compact Flash cards are available with a capacity of :

- 64MB (ROF 157 5126/1)
- 256MB (ROF 157 5126/3)

Remove the transport protection for the hard disk and keep it in case of re-shipment e.g. factory repair. Install and configure the VMU-HD in the cabinet according to the requirements in
Start Of Operation (1537‑ASB 150 02 Uen).

Note

The VMU-HD will not start up without the internal directories created on the hard disk.

##### Board assembling up to Revision
ROF 157 5126/1 R4F and ROF 157 5126/3 R1F

#####

|  | Insert PROM RYS 102 526/2 *) |
|  | Insert PROM RYS 102 526/1 *) |
|  | Press this button to disengage the hard disk and take it out. |

*) part of order number: LZYBS 203 5126

##### Board assembling for Revision
ROF 157 5126/1 R5A and ROF 157 5126/3 R2A

|  | Insert PROM RYS 102 526/2 *) |
|  | Insert PROM RYS 102 526/1 *) |

*) part of order number: LZYBS 203 5126

#### DIP switches

The DIP switch 990 selects whether the register function is enabled or not.

990/1 | 990/2 | Function
OFF | ON or OFF | 16 channels, no register function
ON | OFF | 8 channels with MFC detection and DTMF / Tone receiver
ON | 8 channels with MFE detection and DTMF / Tone receiver

#### Flash disk (prior Hard disk)

The Flash disks will already be pre-configured in the factory with announcements and voice prompts in the proper language (related to the country which has placed the order).

The announcements and the voice prompts can always be adapted according to the customer needs, see document BusinessPhone 250/50 VMU-HD & MFU (1553-ROF 157 5126 Uen).

In case you need another language version than the pre-configured one, please contact your local Ericsson Support Centre

The directory structure on the Flash disk looks as follows:

    \Info0    \message2    \anno0
    \Info1    \message3    \anno1
              \message4    \anno2
              \message5    \anno3
                            :
                         \annoF

To modify the files on the Flash disk use a PC with a PCMCIA drive.

#### Limitations

Only one VMU-HD ( with a PCMCIA Hard disk) can be mounted per cabinet and just one type either VMU-HD or VMU-D can be installed in a system.

Revision: J © Ericsson Enterprise 2005