BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2172
Gatekeeper identifier

In order to distinguish between the different installed Gatekeepers on the customer’s LAN, this command is used to define a unique name (identifier) for each Gatekeeper (according to ITU-T Recommendation H.323.)

The identifier is used for IP-clients and for communication with other gatekeepers (neighbourhood and backup neighbourhood gatekeeper).

If modified, a restart of the IPU is required.

##### Valid data

0-35 |  | characters |
empty (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005