BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0xAC
Battery Backed Up RAM Usage Error

Default definition: |  | ALARM |
Used by block: |  | OS |
Category: |  | DESIGNER |

This warning code indicates an usage error in the battery backed up RAM.

- D1: Type of error

- 01h: Generated by ARRAY.CREATE, if there isn’t enough memory to create a new array.
- 02h: Generated by ARRAY.CREATE, if the requested array already exists, but is of another size.
- 03h: Generated by ARRAY.CREATE, if an existing, ‘incorrect array’ has been recreated.
- 04h: Generated by ARRAY.CHECK, if a non recognized memory gap was found between two arrays.

- D2: 0
- D3: Array identity or number of bytes in memory gab, high byte
- D4: Array identity or number of bytes in memory gab, low byte

Revision: K © Ericsson Enterprise 2005