BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1417
Length of external inquiry signal

The command is used to state the length of the inquiry signal sent via the connected trunk on initiation of inquiry in the interworking exchange.

Value = 002-255, (20-2550 ms)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005