BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1423
Time supervision of B-answer

The command is used for time supervision of answering signal from cooperating exchange. If the cooperating exchange does not answer with this signal there is no use activating this command.

This command is also used for time supervision of answering from ISDN terminals (S-interface). The call is then released.

Value = 0 means no supervision.

Value = 1-255 time supervision in number of seconds.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005