BusinessPhone Communication Platform 7.0
Dialogs

## Transmission – Conference Table

To access the dialog, open the “System” menu in the Configuration directory tree. Next open the “System parameters” submenu and click on “Transmission”. Select “Conference Table” in the context menu.

Attenuation for 3 parties | Selection: 0, 3, 6 or 9 dB
Attenuation for 4 parties
Attenuation for 5 parties
Attenuation for 6 parties

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To load the current system settings. |

See facility description Conference (154/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005