BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8603
Guest extension welcome 2

Each welcome announcement consists of two parts. The first part is always played when a call is diverted to the individual mailbox system (see command 8601 Guest extension welcome 1). If the directory number of the extension is to be played (see command 8602 Announce directory number 0?), the second part of the welcome announcement is played as well. This welcome message is used when a guest extension is diverted to the individual mailbox system. Three different languages can be stated in the hotel system (see command 8009 Wake-up language 1-8011 Wake-up language 3). In this command it is possible to play a separate welcome announcement for each language.

To play the directory number as well, digits for all three languages must have been recorded according to commands 4419 Digits-4421 Digits – language 3.

In this command the reference number for the second part of the welcome message is stated. For the first part see command 8601 Guest extension welcome 1.

The reference is supposed to have been recorded according to command 4415 Welcome individual. Note that recording in command 4415 is only possible on a VMU-HD board.

##### Valid data

0-31 |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005