BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0xC0
Switch TX-Level Error

Default definition: |  | ERROR + TRIG |
Used by block: |  | SX |
Category: |  | DESIGNER |

The SX-block has detected some error, related to its handling of transmission levels.

- D1: Type of error

- 00H ... RP ordered to listen to a reserved PCM channel, order not executed.
- 01H ... RP ordered to send on a reserved PCM channel, order not executed.
- 02H ... RP ordered to send on a channel, where already one sender active, order is executed.
- 03H ... SX is ordered to adjust the transmission for a RP, connected to the silent channel, order not executed.

- D2: PCM-channel

- Bit 0 - 5 ... Timeslot
- Bit 6 ... PCM-bus
- Bit 7 ... Not used

- D3: Type of received message

- 00H ... Not specified
- 01H ... TRANSM,TRMREP
- 02H ... TRANSM,TRMCONSPK
- 03H ... TRANSM,TRMCONREQ
- 04H ... TRANSM,TRMCONNOM
- 05H ... TRANSM,TRMCONADJ
- 06H ... SXCNFCHANGE, SXCNFADD (SX-internal message)
- 07h ... SXCNFCHANGE, SXCNFREMOVE (SX-internal message)
- 08H ... SXCNFREL (SX-internal message)

- D4: Sender of message (ST)

Revision: K © Ericsson Enterprise 2005