BusinessPhone Communication Platform 7.0
Dialogs

## Tone Fragments

Tone fragments are components of tones. Depending on the number of DTMF-tones there can be 19 or 15 fragments.

Command | Value
Frequency 1 (Hz) | Value Range: 300-3400 Hz
Level 1 (dBm0) | Value Range: -64.0-3.0 dB (Step: 0.5 dB)
Frequency 2 (Hz) | Value Range: 300-3400 Hz
Level 2 (dBm0) | Value Range: -64.0-3.0 dB (Step: 0.5 dB)

To access the dialog, open the “System” menu in the Configuration directory tree view. Then open the “System” submenu and open the “Ring & tone signals” option. Now click on “Tones...” to view the context menu. Select “Tone fragments”.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

See facility description Ring And Tone Signals (443/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005