BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2165
Voice Transmission Quality Table 1

The voice transmission quality tables 1-4 are defining in which order the different voice codes shall be accessed according to their availability in case of call setups to an IP network as well as to an IP-Extension. The commands 2165-2168 are used to re-arrange the order according to the customer’s needs.

Each extension can be assigned to one of the four voice transmission tables, see command 0188 Voice transmission quality.

##### Default order

1 |  | G.711 (A-law) |
2 |  | G.711 (m-law) |
3 |  | G.723.1 |
4 |  | G.729 Annex A with Annex B |
5 |  | G.729 Annex A |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005