BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8008
Wake-up ring attempts

The system has an integrated function for waking up guests. On wake-up the guest is rung by the system.

By commands 8006 Wake-up ring time-8008 Wake-up ring attempts the following parameters can be determined for the wake-up call:

- Ringing duration of each wake-up attempt (1-59 s)
- Length of the pause between the wake-up attempts (1-5 minutes)
- Number of wake-up attempts (1-5)

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005