BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x0C
Load Regulation Queue Full

Default definition: |  | UNDEFINED |
Default limit: |  | 65000 |
Used by block: |  | OU |
Category: |  | DESIGNER |

This warning is sent, when there are no more free positions in the load regulation queue, handled by OU.

- D1: Current number of used queue positions.
- D2: Maximum number of available positions (size of queue).
- D3: User identity, ST or CARD.
- D4: User identity, SN or IND.

Revision: K © Ericsson Enterprise 2005