BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1607
Call meter type

The command is used to state the type of the charging pulse receiver for connection to the external line.

Call metering is done on the BTU device board and reception can be done if the analogue trunk is equipped with a daughter board, CM 12 or CM 12/16 (charging receiver) for call metering.

Trunk individuals using the same daughter board, CM 12/16, shall be programmed with the same values for command 1607 Call meter type and command 1608 Call meter receiver level.

Charging with 50 Hz receiver is not affected by this command.

Value = 12 or 16 (12 kHz or 16 kHz)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005