BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2085
PBX protocol identifier

The command defines the PBX protocol identifier for this node in the network. The protocol identifier is used to identify proprietary network calls and services.

Value = ( 0-FFh )

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005