BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3834
Select minutes or seconds for overflow time

This command defines whether the value programmed in command 3825 Overflow time is interpreted as minutes or as seconds.

##### Valid data

MINUTES |  | (Default) |
SECONDS |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005