BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2613
Signal time

This command defines the tone time in ms per digit for digit sending with DTMF.

Value: 0-65535

Initial value = 70

Note

Tone time = 65535 means continuous tone sending (of first keyed digit). Intended for use when measuring the DTMF-signal.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005