BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2505
Abbreviated number category 3

This command defines whether or not the abbreviated number shall be available for the abbreviated number category 3.

Y = Open for category |  |

N = Blocked for category (default data) |  |

An existing abbreviated number is erased by pressing the “-” -key on the phone. This key can also be used as backspace during programming of an abbreviated number.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005