BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8422
Authority code

This command is used to specify the authority code of a tenant. This authority code (up to 16 digits) will be sent to the carrier if specified in command 8415 Arranging number to send.

For every digit you type, a star is displayed. Since the code cannot be read out, it is recommended to enter always the complete code.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005